STM32CubeMX

Table Of Contents

- STM32CubeMX documentation
- CubeMX User Manual
  - 1 STM32Cube overview
  - 2 Getting started with STM32CubeMX
  - 3 Installing and running STM32CubeMX
  - 4 STM32CubeMX user interface
  - 5 STM32CubeMX tools
  - 6 STM32CubeMX C Code generation overview
  - 7 Code generation for dual-core MCUs (STM32H7 dual-core product lines only)
  - 8 Code generation with TrustZone enabled (STM32L5 series only)
  - 9 Device tree generation (STM32MPUs only)
  - 10 Support of additional software components using CMSIS-Pack standard
  - 11 Tutorial 1: From pinout to project C code generation using an MCU of the STM32F4 series
  - 12 Tutorial 2 - Example of FatFs on an SD card using STM32429I-EVAL evaluation board
  - 13 Tutorial 3 - Using the Power Consumption Calculator to optimize the embedded application consumption and more
  - 14 Tutorial 4 - Example of UART communications with an STM32L053xx Nucleo board
  - 15 Tutorial 5: Exporting current project configuration to a compatible MCU
  - 16 Tutorial 6 - Adding embedded software packs to user projects
  - 17 Tutorial 7 - Using the X-Cube-BLE1 software pack
  - 18 Creating LPBAM projects
  - Appendix A STM32CubeMX pin assignment rules
  - Appendix B STM32CubeMX C code generation design choices and limitations
  - Appendix C STM32 microcontrollers power consumption parameters
  - Appendix D STM32Cube embedded software packages
  - Revision history
- Release Notes
  - Release details
  - Release fixes
  - Known limitations
    - Miscellaneous
    - 2.1. When selecting microcontrollers in the STM32C0 series
    - 2.2. When selecting microcontrollers in the STM32G0 series
    - 2.3. When selecting microcontrollers in the STM32G4 series
    - 2.4. When selecting microcontrollers in the STM32H5 series
    - 2.5. When selecting microcontrollers in the STM32H7 series
    - 2.6. When selecting dual-core microcontrollers in the STM32H7 series
    - 2.7. When selecting microcontrollers in the STM32L5 series
    - 3.4. How to improve the wake-up from Stop sequences without relying on the global SystemClock_Config()
    - 3.3. List pinout-compatible microcontrollers
    - 3.2. DDR binaries for the STM32MP1 boards
    - 3.1. Command line authentication required
    - 2.21. Symbolic links on Ubuntu
    - 2.20. User manual
    - 2.19. DDR test suite
    - 2.18. STM32CubeIDE toolchain
    - 2.13. When selecting microcontrollers in the STM32WL series
    - 2.11. When selecting microcontrollers in the STM32WB series
    - 2.17. When using additional software packs
    - 2.16. When using the Example Selector
    - 2.15. When using the Memory Management Tool
    - 2.14. When selecting microprocessors in the STM32MP1 series
    - 2.11.1. When selecting microcontrollers in the STM32WB0 product lines
    - 2.12. When selecting microcontrollers in the STM32WBA series
    - 2.13.1. When selecting microcontrollers in the STM32WL33 product lines
    - 2.10. When selecting microcontrollers in the STM32U5 series
    - 2.9. When selecting microcontrollers in the STM32U3 series
    - 2.8. When selecting microcontrollers in the STM32N6 series
- Running STM32CubeMX in command-line mode
- FAQ
- Community

# Appendix D STM32Cube embedded software packages

Along with STM32CubeMX C code generator, embedded software packages are part of STM32Cube initiative (refer to DB2164 databrief): these packages include a low-level hardware abstraction layer (HAL) that covers the microcontroller hardware, together with an extensive set of examples running on STMicroelectronics boards (see Figure 758). This set of components is highly portable across the STM32 series. The packages are fully compatible with STM32CubeMX generated C code.

> Figure 758. STM32Cube Embedded Software package

> Note: STM32CubeF0, STM32CubeF1, STM32CubeF2, STM32CubeF3, STM32CubeF4, STM32CubeL0 and STM32CubeL1 embedded software packages are available on st.com. They are based on STM32Cube release v1.1 (other series will be introduced progressively) and include the embedded software libraries used by STM32CubeMX for initialization C code generation.

> The user should use STM32CubeMX to generate the initialization C code and the examples provided in the package to get started with STM32 application development.