STM32CubeMX

Table Of Contents

- STM32CubeMX documentation
- CubeMX User Manual
  - 1 STM32Cube overview
  - 2 Getting started with STM32CubeMX
  - 3 Installing and running STM32CubeMX
  - 4 STM32CubeMX user interface
  - 5 STM32CubeMX tools
  - 6 STM32CubeMX C Code generation overview
  - 7 Code generation for dual-core MCUs (STM32H7 dual-core product lines only)
  - 8 Code generation with TrustZone enabled (STM32L5 series only)
  - 9 Device tree generation (STM32MPUs only)
  - 10 Support of additional software components using CMSIS-Pack standard
  - 11 Tutorial 1: From pinout to project C code generation using an MCU of the STM32F4 series
  - 12 Tutorial 2 - Example of FatFs on an SD card using STM32429I-EVAL evaluation board
  - 13 Tutorial 3 - Using the Power Consumption Calculator to optimize the embedded application consumption and more
  - 14 Tutorial 4 - Example of UART communications with an STM32L053xx Nucleo board
  - 15 Tutorial 5: Exporting current project configuration to a compatible MCU
  - 16 Tutorial 6 - Adding embedded software packs to user projects
  - 17 Tutorial 7 - Using the X-Cube-BLE1 software pack
  - 18 Creating LPBAM projects
  - Appendix A STM32CubeMX pin assignment rules
  - Appendix B STM32CubeMX C code generation design choices and limitations
  - Appendix C STM32 microcontrollers power consumption parameters
  - Appendix D STM32Cube embedded software packages
  - Revision history
- Release Notes
  - Release details
  - Release fixes
  - Known limitations
    - Miscellaneous
    - 2.1. When selecting microcontrollers in the STM32C0 series
    - 2.2. When selecting microcontrollers in the STM32G0 series
    - 2.3. When selecting microcontrollers in the STM32G4 series
    - 2.4. When selecting microcontrollers in the STM32H5 series
    - 2.5. When selecting microcontrollers in the STM32H7 series
    - 2.6. When selecting dual-core microcontrollers in the STM32H7 series
    - 2.7. When selecting microcontrollers in the STM32L5 series
    - 3.4. How to improve the wake-up from Stop sequences without relying on the global SystemClock_Config()
    - 3.3. List pinout-compatible microcontrollers
    - 3.2. DDR binaries for the STM32MP1 boards
    - 3.1. Command line authentication required
    - 2.21. Symbolic links on Ubuntu
    - 2.20. User manual
    - 2.19. DDR test suite
    - 2.18. STM32CubeIDE toolchain
    - 2.13. When selecting microcontrollers in the STM32WL series
    - 2.11. When selecting microcontrollers in the STM32WB series
    - 2.17. When using additional software packs
    - 2.16. When using the Example Selector
    - 2.15. When using the Memory Management Tool
    - 2.14. When selecting microprocessors in the STM32MP1 series
    - 2.11.1. When selecting microcontrollers in the STM32WB0 product lines
    - 2.12. When selecting microcontrollers in the STM32WBA series
    - 2.13.1. When selecting microcontrollers in the STM32WL33 product lines
    - 2.10. When selecting microcontrollers in the STM32U5 series
    - 2.9. When selecting microcontrollers in the STM32U3 series
    - 2.8. When selecting microcontrollers in the STM32N6 series
- Running STM32CubeMX in command-line mode
- FAQ
- Community

# 2.12. When selecting microcontrollers in the STM32WBA series

Creating a new project with an STM32WBA microcontroller, enabling BLE in the STM32_WPAN middleware, and generating the build files using CMake or Makefile may result in a compilation error due to the reversed linking order of the libraries `stm32wba_ble_stack_full.a` and `WBA5_LinkLayer_BLE_Full_lib.a`.

To solve the issue, reverse the order of the two libraries in the Makefile or CMake configuration.

The execution in EWARM or KEIL IDEs of an STM32WBA project enabling TrustZone and configuring GTZC/SAU may fail due to a linker files mismatch.

To resolve this issue, manually update the RAM address definitions in the linker files for WBA5/WBA5M and WBA6/WBA6M devices.

Some unexpected behaviors might appear during the creation of an STM32WBA63 project: a non-updated STM32_WPAN Advertising elements menu, erroneous warnings at the peripheral configuration, and failures of IOC file reopening that lead to STM32CubeMX’s home screen.

When the selected middleware is STM32WPAN for Bluetooth® Low Energy with the parameter `CFG_BLE_NUM_LINK` set above 8, use the Bluetooth® Low Energy link layer library `LinkLayer_BLE_Basic_20_links_lib.a` with the corresponding header file.

When building the BLE_Audio_TMAP_Central example for the STM32WBA55G-DK1 in STM32CubeIDE after being processed by STM32CubeMX, some library files might be missing or incorrectly referenced, leading to build errors.

To ensure proper library inclusion after installing the example: - Enable Library Copying. - Or manually update paths in the `.extSettings` file.